Instruction for System C

(This instruction is assumed to run on Windows system to run bat file.)  
**1. To start the system:**1-1.       Open command prompt window  
1-2.       Open SystemC folder  
1-3.       Type **Start.bat** on command prompt window and hit Enter.  
1-4.       When a message that “Starting ECS system” is appeared, then hit Enter key.  
1-5.       Then, original system consoles will be appeared on a screen.  
1-6.       To operate security system, hit Enter key again on the command prompt window.  
1-7.       Then, console windows related to security system will be appeared on the screen.

1-8. When a message that “Starting Security Maintenance System…” is appeared, then hit Enter key. Then, the maintenance system console windows will be appeared.

2. To operate System C:

2-1 The red/green light indicators indicate if a sensor is off- or online. A red light means the sensor is offline, a green light means it is online.

2-2 The default checking period is set to 5 seconds.

2-3 Delays in the event manager may cause delays when detecting if a sensor is online or offline

2-4 To test the maintenance console, simply end the process of the sensor that you wish to take offline.

2-5 The light indicator of the sensor that was taken down will be updated to red after a couple of seconds.